New Device to On-Board


Open Access to the Serial PORT on the linux server
- Create a File /etc/udev/rules.d/99-serial.rules
- Paste inside KERNEL=="ttyUSB[0-9]*",MODE="0666"


Check if you can see the USB device
    - ls -lA /dev/serial/by-id
Configure the Scanner Manually using the Barcode Scanner using the RS232 Barcode Setting.
